Specification for Tackboard Series

PRODUCT: Tackboard

SECTION XXXXX – TACKBOARD PANELS
PART 1  -  GENERAL
1.1
SUBMITTALS


A.
Product Data:
I. Manufacturer Specifications and other data needed that provides proof of compliance with specified requirements.



II.
Submit quantity of _______ vinyl selector cards from manufacturer’s 



standard finishes, or designer specified finishes.



III.
Include appropriate technical information including test data and 




maintenance instructions.

B.
Shop Drawings:
I. Show panel joints, detail references, dimensions and method of attachment.

C. Samples:

I.
Submit 12 inch x 12 inch sample of actual material and color cards showing manufacturer’s full range of colors for Architect’s selection.



II.
Submit quantity of _______ samples of each type of panels as shown on 


the drawings and in schedules. 


D.
Substitutions or changes to this specification will only be permitted by prior 


approval by the architect.
1.2
QUALITY ASSURANCE

A.
Single Source Responsibility: Obtain panel materials from a single 



manufacturer. Provide panels and vinyls of each type required from 



one (1) manufacturer, of uniform texture and color.

B. Installer to provide evidence of appropriate experience in system installation and that installation method proposed is acceptable to panel manufacturer. 

1.3
DELIVERY, STORAGE AND HANDLING
A.
Carefully protect products during shipment, storage and installation.

B.
Deliver materials to job site in unopened packages or crates and store elevated 


above floor in an enclosed space with proper ventilation and protection from 


damage.

PART 2  -  PRODUCTS
2.1
ACCEPTABLE MANUFACTURERS

A. Lamvin, Inc. (http://www.lamvin.com)

4675 North Ave. Oceanside, CA 92056

(800) 446-6329 (Phone)

(760) 806-3200 (Fax)

sales@lamvin.com 


B.
Manufacturer substitutions are not permitted

2.2
MATERIALS

A. Panels shall be Lamvin’s Tackboard Wall Panels as manufactured by Lamvin, Inc. 4675 North Avenue, Oceanside, CA 92056 | Phone (800) 446-6329, Fax (760) 806-3200. 


B. 
Tackboard panels shall be constructed of a compressed industrial insulation 


wood fiberboard. Thickness shall be 1/2”. 

C. 
Sizes: Shall be 4 feet wide by ________ high or as shown on drawings. 



Panels are to be manufactured according to field dimensions supplied by the 


installing contractor. Standard tolerances are ± 1/16” in width and height.

D. 
Edge Profile: Shall be Square. Corner Detail: Shall be Square.

E.
Vinyl Finish: Finish shall be Koroseal’s “School Collection” in colors selected by 


Architect from Manufacturer’s full range of colors, or _____________________ 


______________________ (specify). Finish shall be applied directly to face and 


long edges of the panel and returned onto the back of the panel. 

F. 
Mounting: Shall be OSI GreenSeries Drywall Panel Construction Adhesive.

G.
Trim: Provide ________ linear feet of vinyl covered F-Mold Trim (Outside Corner), ________ linear feet of vinyl covered Z-Mold Trim (Inside Corner) or according to quantity requested by the installing contractor. 


 H.
Extra Materials: Provide 5% additional material for use by owner for building 


maintenance and repair. 

PART 3  -  EXECUTION

3.1 INSPECTION

A.
Verify dimensions to ensure proper fabrication of materials.

B. The contractor shall be responsible for the examination and acceptance of all surfaces and conditions prior to the acoustical panel installation.
3.2 INSTALLATION

A. Installation of panels shall not begin until all wet work (plastering, concrete, etc.) is completed and dry. Building shall be properly enclosed and under standard occupancy conditions (temperature of 60-85° F and not more than 70% relative humidity) before installation begins.
B.
Install panels and fabrics in accordance with manufacturer’s instructions and 
approved shop drawings.

C. Arrange panels symmetrically on each wall, unless otherwise indicated. 

D. Arrange panels and orientate directional pattern, if any.

E. Remove panels that are damaged and unacceptable to Architect and replace with new undamaged materials at no expense to owner.
F. Do not begin installation until unacceptable conditions are corrected.
END OF SECTION XXXXX
To download this specification, please visit http://www.lamvin.com
